IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "ee2fb7aa-528a-431c-9783-af44dfcc1cea.ifc"
Time stamp: "2021-01-18T11:52:49"
Author: "BouwConnect Bibliotheek"
Organization: "De Twee Snoeken"
Preprocessor: "IFC Engine DLL"
Originating system: "BouwConnect Bibliotheek"
Authorization: "De Twee Snoeken"
Application: "BouwConnect Bibliotheek" version "1.0" identifier "BouwConnect Bibliotheek" by Organization "BouwConnect Bibliotheek" description "BouwConnect Bibliotheek"

People and organizations
  Person "webapp.bcbplaat" of Organization "BouwConnect Bibliotheek" description "BouwConnect Bibliotheek"
  Owner history of Person "webapp.bcbplaat" of Organization "BouwConnect Bibliotheek" description "BouwConnect Bibliotheek" | application "BouwConnect Bibliotheek" version "1.0" identifier "BouwConnect Bibliotheek" by Organization "BouwConnect Bibliotheek" description "BouwConnect Bibliotheek" | change ADDED | created 1610970766 (2021-01-18T11:52:46Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  SOLIDANGLEUNIT: STERADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "afvoerput Aquaberg - vloerafvoerput 146x146mm onderaansluiting"
  IFCSITE "Kavel" | latitude 0° 0′ 0″ | longitude 0° 0′ 0″ | elevation above sea level 0.
    IFCBUILDING "Gebouw" | postal address: "Gebouw"
      IFCBUILDINGSTOREY "Bouwlaag" | elevation 0.
        contains 1 element
          1 x IFCFLOWTERMINAL | material: "RVS" | property sets: Pset_Data

Property sets
  Pset_Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Hyperlink = "https://bcb-online.nl/s/050bfc0e5bf844f30bd870719b74933bb" (IFCTEXT)
    STABU2 = "51.42.10" (IFCTEXT)
    WUID = "AgAAAPVr5VUDAAAAexoAAAWggwAAvEYBALtzAADXGQAAJeoBAAIAMAcBAQAAAAEAAADoAQEBAAAAAgAAAPdRAAAFzRwAAGQwAADGpwAAo60AAOnYAAAAAOw_AAAFeLkAAGQwAADGpwAAo60AAOnYAAABAO8EAgQIQUlTSSAzMDQ)" (IFCTEXT)
    aansluiting = "onderaansluiting, spie-end" (IFCTEXT)
    artikelnummer = "4015146" (IFCTEXT)
    breedte = "146" (IFCTEXT) [mm (context dependent)]
    diameter aansluiting = "50" (IFCTEXT) [mm (context dependent)]
    eenheid = "st" (IFCTEXT)
    inbouwdiameter = "162" (IFCTEXT) [mm (context dependent)]
    kenmerkende grondstof = "RVS" (IFCTEXT)
    lengte = "146" (IFCTEXT) [mm (context dependent)]
    merk = "Aquaberg" (IFCTEXT)
    nominale uurcapaciteit = "3600" (IFCTEXT) [l/h (context dependent)]
    puthuis = "ABS" (IFCTEXT)
    rooster = "RVS" (IFCTEXT)
    serie = "vloerafvoerput" (IFCTEXT)
    uitvoering = "onderaansluiting" (IFCTEXT)